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	Model
	R9K-1200

	Internal Dimensions (mm)
	1000*1200*1000

	Overall Dimensions (mm)
	1250*1700*2050

	Interior Volume (L)
	1200

	Parameter
	Water Spray Angle
	0°, 30°, 60°, 90°

	
	Water Spray Temperature
	Ambient ~ +88℃ (Adjustable)

	
	Spray Nozzle
	Four, 30 Seconds each position

	
	Distance from Water Spraying to Specimens
	10~15cm

	
	Water Pressure
	8000-10000 Kpa (Adjustable)

	
	Water Flow Rate
	14L-16L/min

	
	Testing Platform Speed
	5±1 r.p.m

	
	Testing Platform Height
	200-400 nm (Adjustable)

	
	Testing Platform Diameters
	600mm

	Structure
	Temperature Sensor
	PTR Platinum Resistance PT100Ω/MV A-class

	
	Heater Elements
	Nichrome heater

	
	Controller
	Programmable color LCD touch screen controller

	
	
	Ethernet connection, PC Link, USB

	
	Build-in Water Tank(mm)
	370*375*950

	
	View Window Size(mm)
	475*475

	
	Door Lock
	Electromagnetic lock

	
	Water supply system
	Storage water tank; Booster pump; Automatic water supply; Water purification system;

	
	Safety Device
	Over-temperature Protection; Over-current Protection; 

Water Shortage Protection; Earth leakage Protection; Phase Sequence Protection

	Material
	Exterior Material
	Steel Plate with protective coating

	
	Interior Material
	SUS304 stainless steel

	
	Observation Window
	 Double layer insulating glass with wiper

	Power Supply
	380V 50Hz

	Maximum Noise

	65 dBA

	Environmental Conditional
	5℃～+35 ℃   40%~85% RH

	Standard
	IEC 60529; ISO20653; DIN 40050-9; USCAR-2; GMW-3191
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At present 7 Tier-one agents around the world provide LIB products, installation and maintenance service for customers. Make things simple and convenient.  
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XI'AN LIB ENVIRONMENTAL SIMULATION INDUSTRY


Climatic Test Chamber Manufacturer and Supplier 








IPX9K High Pressure Water Spray Test Chamber  


                                                


                                                 








Structures





Temperature & Humidity Test Chamber





IP Rate


IPX9K





Water Spray Temperature


Ambient ~ +88℃





Water Spray Pressure


8000-10000Kpa





Automobile industry








Electronics








Military








R9K-1200





IPX9K High Pressure Water Spray Test Chamber








【Technical Parameter】








Standard & customized


* pay attention to the environmental condition during installing


Automatic water supply ensures adequate supply of water and automatic testing.








The controller is diversity designed,It can communication with LAN network interface by R-232 /R-485interface.


* pay attention to the environmental condition during installing








It can cool down to -86℃.


The Refrigerant can be replaced by R449A/R508B for Europe market.


The heat load can Absorbs 1000w in -20℃.














Structures





IPX9K High Pressure Water Spray Test Chamber








Appearance
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Safety protect system








Over Temperature Protection


Water Shortage Protection


Over Current Protection


Earth Leakage Protection


Phase Sequence Protection
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1.Workroom








4.Viewing Window 








7.Castor  








Install 4 castors for easy to move, and with brakes function. Caster height is adjustable.








The internal material is 304 stainless steel, mirror surface, rust-proof, high temperature and corrosion resistance;


Nice ruggedness and long life.


The workroom is equipped with a single-phase 16A internal power interface to power up the test specimen. The power-on time and cycle can be controlled by the controller.








Double-layer tempered glass, specially designed seal, with good impact resistance and prevention of water leakage.


Equipped with manual water wiper for easy observation samples.

















8.Water Re-circulation





Water purifier: mainly purification from water source to water tank.


Water re-circulation system that reduced water use and a series of water pipes





5.Build-in Lighting





The built-in waterproof LED lighting inside the workroom makes it clear to observe the test specimen. The light can be turned on and off at the control panel button.














2.Spray Nozzles





There are four nozzles, and the samples can be placed at four angles (0 °, 30 °, 60 °, 90 °) for high temperature and high pressure water jetting test.





9.Automatic Water Inlet 








Automatic control of the water intake of equipment, the customer can be directly connected to the laboratory faucet, so as to achieve automated testing;


Automatic inlet diameter 1/2 inch (13.5MM);


High and low water level alarm, water shortage lights and sound.


Standard 2 meter drain pipe.








6.Controller  








PID programmable color touch screen controller, network connection computer.


Can edit 100 programs 20 segment..


LIB also can preset program into the controller based on user testing requirements.


The set system language is English for standard.








3.Turntable 





The turntable is made of 304 stainless steel, the speed and angle can be adjusted.


Sample should be firmly fixed on the turntable.





10.External Materials 








A3 steel plate with galvanized coating;


Electrostatic treatment; High and low temperature corrosion resistance; High hardness, anti - impact


Very high safety factor;


Color can be customized.





IPX9K Water Spray Test Chamber





Option





Reverse Osmosis Unit








Demineralized Water Device





WiFi connection


Mobile APP control


Multi-language controller interface：Russian,


French, Polish, Romanian, German

















Controller











Shipping & Packaging





Install Condition





      Environment Conditions


Temperature: +5°C ~ +35°C


Relative humidity: ≤85%;


Pressure: 86 KPa—106 KPa








Space Conditions


Sufficient space for ventilation








*Safety Instruction：1.Prohibited to test explosive, inflammable and high corrosive substance�2.Chemical exposure to the equipment is prohibited�3.Equipment must be safety on the ground to avoid electrostatic induction








Packaging











Plywood: standard wood export packaging.


The wooden box is fixed by sheet metal to 


prevent damage during transportation.





Gross weight: 800kgs~	


Package size: 5.08CBM








First, seal chamber with waterproof plastic film.


Protect chamber from seawater corrosion.


Second, buffer foam is placed in the four 


corners of the chamber.It is used for fixing


equipment to prevent shaking and damaging 


chamber during transportation.








Shipping








+ 





Material：Export standard wooden box 


*Can be used for Sea, Air, Railway, Truck and


 multimodal transport.








Warranty & Service 


- 3 Years Warranty, Lifelong Follow-up Services





Professional After-sales Team


If you have any questions during operation,


we will supply solution to you with 24 hours.











Environment conditions


Temperature: +5°C ~ +35°C


Relative humidity: ≤85%;


Pressure: 86 KPa—106 KPa








How to Service





1. At first, our test chambers are produced based on 20 years product lifetime. 


Normally once test chambers have problems, we judge the problems, and send spare parts to our customers, and teach them how to change new parts on by email or video, all spare parts and shipping cost (by DHL, TNT, and FedEx) paid by LIB. 


2. If the customer needs our engineer on-site service, they only need pay the ticket accommodation to our Engineers, service is for free.


3. If products still can't use after our engineers repair, we will produce a new test chamber (same as the old one) to our customers with no charge. 














    Our company will repair the product, if the product, the material of the parts, the design and manufacturing of the products raised hardware problems caused by product itself rather than human error within three years warranty period since the date of dispatching by the customer. 


Our company repairs the products, but will collect the basic costs of the spare parts after the warranty period, but service is free always. 








Warranty Condition 








LIB Industry®








         





         





         





         





         





         





         





         





         





PARTNER 





         





         





         





Xi’an LIB Environmental Simulation Industry








PROVIDING TEST SOLUTION, PROVIDING TEST EQUIPMENT








CE 


ROHS








Xi’an LIB Environmental Simulation Industry is a lead provider of environmental test chamber in China, with its own brand (LIB) design, production, sales and service since 2009. We continually update technology and develop new products for customer’s needs.


Our main products included temperature and climate test chambers, corrosion chambers, weathering testers, IP dust and rain chambers, ozone test chamber, noxious gas SO2 H2S chamber, walk-in chambers. We provide test chamber, we provide test solution. Standard and customized products to meet different customer needs.


By 2018, global market has spread to 53 countries to USA, Canada, Mexico, Brazil, Peru, Russia, German,UK,France,Finland,Netherlands, Poland,Switzerland,Thailand,Philippines, Singapore, Malaysia, Australian, South Africa etc. and the market continues to expand.








LIB became a registered trademark of our company since 2017 year.





Contact Us


Website: www.lib-industry.com


Add: No.5 Zhangba First St, Xian High-Tech Area, Shaanxi ProvinceP.R.China  710065


Tel: +86 29 68918976  


WhatsApp: +86 18700875368 


Skype: serena_lib


Email: serena@ lib-industry.








Sales Team: � HYPERLINK "mailto:sales@lib-industry.com" �sales@lib-industry.com� 


After Sales Team：asd@lib-industry.com


Shipping Team：vip@lib-industry.com


Finance Team：account@lib-industry.com











